## Uses of Class
tw.com.prolific.pl2303multilib.PL2303MultiLib.FlowControl

- - ### Uses of PL2303MultiLib.FlowControl in tw.com.prolific.pl2303multilib

    Methods in tw.com.prolific.pl2303multilib that return PL2303MultiLib.FlowControl
    Modifier and Type | Method and Description
    --- | ---
    `static PL2303MultiLib.FlowControl` | PL2303MultiLib.FlowControl.`valueOf(java.lang.String name)` Returns the enum constant of this type with the specified name.
    `static PL2303MultiLib.FlowControl[]` | PL2303MultiLib.FlowControl.`values()` Returns an array containing the constants of this enum type, in the order they are declared.

    Methods in tw.com.prolific.pl2303multilib with parameters of type PL2303MultiLib.FlowControl
    Modifier and Type | Method and Description
    --- | ---
    `boolean` | PL2303MultiLib.`OpenDevByUARTSetting(int index, PL2303MultiLib.BaudRate R, PL2303MultiLib.DataBits D, PL2303MultiLib.StopBits S, PL2303MultiLib.Parity P, PL2303MultiLib.FlowControl F)` Deprecated. As of PL2303HXD MultiLib_v0.0.1.20, replaced by `PL2303MultiLib.PL2303OpenDevByUARTSetting(int index, BaudRate R, DataBits D, StopBits S, Parity P, FlowControl F)` Open an PL-UART USB Device by UART setting
    `boolean` | PL2303MultiLib.`PL2303OpenDevByUARTSetting(int index, PL2303MultiLib.BaudRate R, PL2303MultiLib.DataBits D, PL2303MultiLib.StopBits S, PL2303MultiLib.Parity P, PL2303MultiLib.FlowControl F)` Open an PL-UART USB Device by UART setting
    `int` | PL2303MultiLib.`PL2303SetupCOMPort(int index, PL2303MultiLib.BaudRate R, PL2303MultiLib.DataBits D, PL2303MultiLib.StopBits S, PL2303MultiLib.Parity P, PL2303MultiLib.FlowControl F)` Setup basic communication parameters on PL2303HXD chip
    `int` | PL2303MultiLib.`setup(int index, PL2303MultiLib.BaudRate R, PL2303MultiLib.DataBits D, PL2303MultiLib.StopBits S, PL2303MultiLib.Parity P, PL2303MultiLib.FlowControl F)` Deprecated. As of PL2303HXD MultiLib_v0.0.1.20, replaced by `PL2303MultiLib.PL2303SetupCOMPort(int index, BaudRate R, DataBits D, StopBits S, Parity P, FlowControl F)` Setup basic communication parameters on PL2303HXD chip